void loop() {

static bool spacePrinted = false; // Flag to track if space has been printed

if (!spacePrinted) {

Serial.println(" "); // Print a space character

spacePrinted = true; // Set the flag to true to indicate space has been printed

}

}

==========================================

Set the (Serial\_Monitor) to “no line ending”

Baud-Rate : Baud\_in\_Code = Baud\_in\_SerialMonitor